Ethernet Connection.txt
=======================

Connecting between PTS Terminal and a PTS system via ethernet
requires both the PC and PTS to be configured correctly.

This document outlines what is necessary for this connection,
however this should be taken as a guide only and cannot
explain particular configurations of Ethernet networking.

Please see your system administrator before changing any
settings on your PC.

Configuration of PC.
====================

The PC will require TCP/IP networking installed, and a suitable
network card for 10Mbps Ethernet.

Once this is installed the PC will require an Ethernet address
for the LAN (local area network) binding of TCP/IP.  This may
form part of the configuration of your companies network.

To check current settings open a "DOS" or "Command" prompt and
type

IPCONFIG /ALL<return>.

The output from this will look 
something like:

Windows 98 IP Configuration

	Host Name . . . . . . . . . : Laptop.Quin42
	DNS Servers . . . . . . . . : 192.168.200.11
	Node Type . . . . . . . . . : Broadcast
	NetBIOS Scope ID. . . . . . : 
	IP Routing Enabled. . . . . : Yes
	WINS Proxy Enabled. . . . . : No
	NetBIOS Resolution Uses DNS : Yes

0 Ethernet adapter :

	Description . . . . . . . . : PPP Adapter.
	Physical Address. . . . . . : 44-45-53-54-00-00
	DHCP Enabled. . . . . . . . : Yes
	IP Address. . . . . . . . . : 0.0.0.0
	Subnet Mask . . . . . . . . : 0.0.0.0
	Default Gateway . . . . . . : 
	DHCP Server . . . . . . . . : 255.255.255.255
	Primary WINS Server . . . . : 
	Secondary WINS Server . . . : 
	Lease Obtained. . . . . . . : 
	Lease Expires . . . . . . . : 

1 Ethernet adapter :

	Description . . . . . . . . : FE575 Ethernet Adapter
	Physical Address. . . . . . : 00-50-DA-84-F7-90
	DHCP Enabled. . . . . . . . : No
	IP Address. . . . . . . . . : 192.168.200.90
	Subnet Mask . . . . . . . . : 255.255.255.0
	Default Gateway . . . . . . : 192.168.200.11
	Primary WINS Server . . . . : 
	Secondary WINS Server . . . : 
	Lease Obtained. . . . . . . : 
	Lease Expires . . . . . . . : 

The adapter that will be used is the Ethernet Adapter (LAN)
and in this case has an IP address of 192.168.200.90

Other adapters will be listed (in this case a modem dial up
PPP adapter) - these will not be used.

To change settings on the PC you will need to change parameters
in the TCP/IP properties (a "protocol") - and reboot the PC.
{Detailed explanation of changing network properties can be
found in the Windows help system, or preferably ask your
system administrator}

Configuration of PTS
====================

The PTS system needs to have an IP address on the same subnet
as the PC.  In the case of the example above this would be
192.168.200.xxx where xxx is a number between 1 and 250, and
is not already used on the network.  Please be careful about
this.

Connect to the PTS unit using a serial cable and PTS Toolkit.
Use the CF command to set the IP address into the PTS system
and then reboot the PTS system.

Cabling between PC and PTS
==========================

This forms a guide only - consult your network administrator.
For a one-to-one connection a twisted pair (UTP) cross-over
cable can be used between the PC and the PTS.  Alternatively
a network hub can be used with two twisted pair (UTP) cables.

Testing the connection
======================

On the PC run a "DOS" or "command" prompt and type:

PING /t 192.168.200.101<return>

(or whatever address the PTS is)

There should be a reply to this.  If not check IP addresses
and and indicator lights on the PTS and ethernet hubs etc.
For more information use the NS command on the PTS (connect
via a serial lead) and the STAT option.

Once PING is working then there is a connection between the
two systems and PTS Toolkit can now be used.

Start PTS Toolkit, create a new Ethernet connection and enter
the appropriate IP address.

Connect and away you go.

Advanced details
================

PTS is capable of routing.  Firewalls and similar can change
port numbers.  Multiple PTS systems can be accessed from one
PC.

Final Warning
=============

Please consult network or system administrator before changing
settings - and be aware that conflicts on ethernet could cause
other users to loose data.

--------------------------------------------------------------
Ethernet Connection.txt
Michael Dye
Quin Systems Ltd.
April 2000