Details on Patch V2.1.0.0 to V2.1.0.1 of PTS Toolkit 2000
---------------------------------------------------------

This patch updates

PTS Editor
PTS Terminal
PTS 'Scope
Q-Drive Setup

With the following changes:

PTS Editor
----------
$CQ=CQ flagged as error by PTS V2.1 parser.  This has
been fixed.

PTS Terminal
------------
When connecting to a SERVOnet axis module the VN detect 
keeps trying even though it is obvious it won't succeed.
This has been changed - the words "Axis Module" are
captured and the VN detect aborts automatically.

PTS ’Scope
----------
When communications are very busy and digital signals 
are being traced the 'scope can sometimes keep asking 
the user to confirm the channel number of digital inputs.  
This only happens if the 'scope trace data is being 
corrupted by continual error messages (e.g. referencing) 
or overloaded serial communications.  The detection of
corrupted trace information has been significantly
improved.

Loading trace data from a LOG file can result in an odd 
display - zoomed in to the start of the trace.  This
has been fixed.

Q-Drive Setup
-------------
When relevant CSV file isn't found for the Q-Drive that 
is being accessed the message box now tells you to 
look to Quins WWW support site, and gives the name of the 
CSV file.  The support WWW site now contains downloadable 
versions of all the CSV files we have produced for 
different versions of Q-Drive. 

When saving a Q-Drive configuration to PC disk a file 
name with more than 39 characters in it causes a 
runtime error, number 5.  This has been fixed.


---------------------------------------------------------
patch.txt
Michael Dye
Quin Systems Ltd.
June 2000